F

A

B

C

G D

E

1. **TOP OF TENT TO TOP OF DOORWAY** 6.5 ft
2. **POLE HEIGHT** 8 ft
3. **DOORWAY HEIGHT** 5 ft
4. **WALL HEIGHT** 3 ft
5. **DIAMETER** 13 ft
6. **AIR VENTS** 4 with mosquito netting
7. **ZIP WINDOWS** 4 with mosquito netting (Note groundsheet not shown on picture above)

**Details**

**Tent** Sides can unzip from groundsheet and tie up – cotton ties Waterproof

**Groundsheet** PVC 540g per sqm

Zips into tent

3.5 “ high but lays flat when unzipped (keeps water out)

Doorway has extra zips to allow doorway section to lay flat when rest of groundsheet is zipped in

Rivetted holes for pegs

**Poles** Galvanised steel Central pole

A-Frame pole for doorway with spike at top of A-frame (with rubber washer round to protect canvas plus riveted hole in canvas)

**Pegs** 24 (groundsheet and guy ropes)

Strong steel – must not bend when hammered

**Guy ropes** 11 & 1 extra long for door

**Carry bag** All contents in a zip carry bag with handle

Bag must be large enough to make packing away easy

**Total weight** 48.5 lbs